Overview | Package | Class | Use | Tree | Deprecated | Index | Help

Java Card
v2.2.2
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## javacard.framework
Interface ISO7816

    public interface ISO7816

`ISO7816` encapsulates constants related to ISO 7816-3 and ISO 7816-4. `ISO7816` interface contains only static fields.

The static fields with `SW_` prefixes define constants for the ISO 7816-4 defined response status word. The fields which use the `_00` suffix require the low order byte to be customized appropriately e.g (ISO7816.SW_CORRECT_LENGTH_00 + (0x0025 & 0xFF)).

The static fields with `OFFSET_` prefixes define constants to be used to index into the APDU buffer byte array to access ISO 7816-4 defined header information.

Field Summary
`static byte` | `CLA_ISO7816` APDU command CLA : ISO 7816 = 0x00
`static byte` | `INS_EXTERNAL_AUTHENTICATE` APDU command INS : EXTERNAL AUTHENTICATE = 0x82
`static byte` | `INS_SELECT` APDU command INS : SELECT = 0xA4
`static byte` | `OFFSET_CDATA` APDU command data offset : CDATA = 5
`static byte` | `OFFSET_CLA` APDU header offset : CLA = 0
`static byte` | `OFFSET_EXT_CDATA` APDU command data offset with extended length input data : EXT_CDATA = 7
`static byte` | `OFFSET_INS` APDU header offset : INS = 1
`static byte` | `OFFSET_LC` APDU header offset : LC = 4
`static byte` | `OFFSET_P1` APDU header offset : P1 = 2
`static byte` | `OFFSET_P2` APDU header offset : P2 = 3
`static short` | `SW_APPLET_SELECT_FAILED` Response status : Applet selection failed = 0x6999;
`static short` | `SW_BYTES_REMAINING_00` Response status : Response bytes remaining = 0x6100
`static short` | `SW_CLA_NOT_SUPPORTED` Response status : CLA value not supported = 0x6E00
`static short` | `SW_COMMAND_CHAINING_NOT_SUPPORTED` Response status : Command chaining not supported = 0x6884
`static short` | `SW_COMMAND_NOT_ALLOWED` Response status : Command not allowed (no current EF) = 0x6986
`static short` | `SW_CONDITIONS_NOT_SATISFIED` Response status : Conditions of use not satisfied = 0x6985
`static short` | `SW_CORRECT_LENGTH_00` Response status : Correct Expected Length (Le) = 0x6C00
`static short` | `SW_DATA_INVALID` Response status : Data invalid = 0x6984
`static short` | `SW_FILE_FULL` Response status : Not enough memory space in the file = 0x6A84
`static short` | `SW_FILE_INVALID` Response status : File invalid = 0x6983
`static short` | `SW_FILE_NOT_FOUND` Response status : File not found = 0x6A82
`static short` | `SW_FUNC_NOT_SUPPORTED` Response status : Function not supported = 0x6A81
`static short` | `SW_INCORRECT_P1P2` Response status : Incorrect parameters (P1,P2) = 0x6A86
`static short` | `SW_INS_NOT_SUPPORTED` Response status : INS value not supported = 0x6D00
`static short` | `SW_LAST_COMMAND_EXPECTED` Response status : Last command in chain expected = 0x6883
`static short` | `SW_LOGICAL_CHANNEL_NOT_SUPPORTED` Response status : Card does not support the operation on the specified logical channel = 0x6881
`static short` | `SW_NO_ERROR` Response status : No Error = (short)0x9000
`static short` | `SW_RECORD_NOT_FOUND` Response status : Record not found = 0x6A83
`static short` | `SW_SECURE_MESSAGING_NOT_SUPPORTED` Response status : Card does not support secure messaging = 0x6882
`static short` | `SW_SECURITY_STATUS_NOT_SATISFIED` Response status : Security condition not satisfied = 0x6982
`static short` | `SW_UNKNOWN` Response status : No precise diagnosis = 0x6F00
`static short` | `SW_WARNING_STATE_UNCHANGED` Response status : Warning, card state unchanged = 0x6200
`static short` | `SW_WRONG_DATA` Response status : Wrong data = 0x6A80
`static short` | `SW_WRONG_LENGTH` Response status : Wrong length = 0x6700
`static short` | `SW_WRONG_P1P2` Response status : Incorrect parameters (P1,P2) = 0x6B00

Field Detail

### SW_NO_ERROR

    static final short SW_NO_ERROR

  Response status : No Error = (short)0x9000

  See Also:
    Constant Field Values

### SW_BYTES_REMAINING_00

    static final short SW_BYTES_REMAINING_00

  Response status : Response bytes remaining = 0x6100

  See Also:
    Constant Field Values

### SW_WRONG_LENGTH

    static final short SW_WRONG_LENGTH

  Response status : Wrong length = 0x6700

  See Also:
    Constant Field Values

### SW_SECURITY_STATUS_NOT_SATISFIED

    static final short SW_SECURITY_STATUS_NOT_SATISFIED

  Response status : Security condition not satisfied = 0x6982

  See Also:
    Constant Field Values

### SW_FILE_INVALID

    static final short SW_FILE_INVALID

  Response status : File invalid = 0x6983

  See Also:
    Constant Field Values

### SW_DATA_INVALID

    static final short SW_DATA_INVALID

  Response status : Data invalid = 0x6984

  See Also:
    Constant Field Values

### SW_CONDITIONS_NOT_SATISFIED

    static final short SW_CONDITIONS_NOT_SATISFIED

  Response status : Conditions of use not satisfied = 0x6985

  See Also:
    Constant Field Values

### SW_COMMAND_NOT_ALLOWED

    static final short SW_COMMAND_NOT_ALLOWED

  Response status : Command not allowed (no current EF) = 0x6986

  See Also:
    Constant Field Values

### SW_APPLET_SELECT_FAILED

    static final short SW_APPLET_SELECT_FAILED

  Response status : Applet selection failed = 0x6999;

  See Also:
    Constant Field Values

### SW_WRONG_DATA

    static final short SW_WRONG_DATA

  Response status : Wrong data = 0x6A80

  See Also:
    Constant Field Values

### SW_FUNC_NOT_SUPPORTED

    static final short SW_FUNC_NOT_SUPPORTED

  Response status : Function not supported = 0x6A81

  See Also:
    Constant Field Values

### SW_FILE_NOT_FOUND

    static final short SW_FILE_NOT_FOUND

  Response status : File not found = 0x6A82

  See Also:
    Constant Field Values

### SW_RECORD_NOT_FOUND

    static final short SW_RECORD_NOT_FOUND

  Response status : Record not found = 0x6A83

  See Also:
    Constant Field Values

### SW_INCORRECT_P1P2

    static final short SW_INCORRECT_P1P2

  Response status : Incorrect parameters (P1,P2) = 0x6A86

  See Also:
    Constant Field Values

### SW_WRONG_P1P2

    static final short SW_WRONG_P1P2

  Response status : Incorrect parameters (P1,P2) = 0x6B00

  See Also:
    Constant Field Values

### SW_CORRECT_LENGTH_00

    static final short SW_CORRECT_LENGTH_00

  Response status : Correct Expected Length (Le) = 0x6C00

  See Also:
    Constant Field Values

### SW_INS_NOT_SUPPORTED

    static final short SW_INS_NOT_SUPPORTED

  Response status : INS value not supported = 0x6D00

  See Also:
    Constant Field Values

### SW_CLA_NOT_SUPPORTED

    static final short SW_CLA_NOT_SUPPORTED

  Response status : CLA value not supported = 0x6E00

  See Also:
    Constant Field Values

### SW_UNKNOWN

    static final short SW_UNKNOWN

  Response status : No precise diagnosis = 0x6F00

  See Also:
    Constant Field Values

### SW_FILE_FULL

    static final short SW_FILE_FULL

  Response status : Not enough memory space in the file = 0x6A84

  See Also:
    Constant Field Values

### SW_LOGICAL_CHANNEL_NOT_SUPPORTED

    static final short SW_LOGICAL_CHANNEL_NOT_SUPPORTED

  Response status : Card does not support the operation on the specified logical channel = 0x6881

  See Also:
    Constant Field Values

### SW_SECURE_MESSAGING_NOT_SUPPORTED

    static final short SW_SECURE_MESSAGING_NOT_SUPPORTED

  Response status : Card does not support secure messaging = 0x6882

  See Also:
    Constant Field Values

### SW_WARNING_STATE_UNCHANGED

    static final short SW_WARNING_STATE_UNCHANGED

  Response status : Warning, card state unchanged = 0x6200

  See Also:
    Constant Field Values

### SW_LAST_COMMAND_EXPECTED

    static final short SW_LAST_COMMAND_EXPECTED

  Response status : Last command in chain expected = 0x6883

  See Also:
    Constant Field Values

### SW_COMMAND_CHAINING_NOT_SUPPORTED

    static final short SW_COMMAND_CHAINING_NOT_SUPPORTED

  Response status : Command chaining not supported = 0x6884

  See Also:
    Constant Field Values

### OFFSET_CLA

    static final byte OFFSET_CLA

  APDU header offset : CLA = 0

  See Also:
    Constant Field Values

### OFFSET_INS

    static final byte OFFSET_INS

  APDU header offset : INS = 1

  See Also:
    Constant Field Values

### OFFSET_P1

    static final byte OFFSET_P1

  APDU header offset : P1 = 2

  See Also:
    Constant Field Values

### OFFSET_P2

    static final byte OFFSET_P2

  APDU header offset : P2 = 3

  See Also:
    Constant Field Values

### OFFSET_LC

    static final byte OFFSET_LC

  APDU header offset : LC = 4

  See Also:
    Constant Field Values

### OFFSET_CDATA

    static final byte OFFSET_CDATA

  APDU command data offset : CDATA = 5

  See Also:
    Constant Field Values

### OFFSET_EXT_CDATA

    static final byte OFFSET_EXT_CDATA

  APDU command data offset with extended length input data : EXT_CDATA = 7

  See Also:
    Constant Field Values

### CLA_ISO7816

    static final byte CLA_ISO7816

  APDU command CLA : ISO 7816 = 0x00

  See Also:
    Constant Field Values

### INS_SELECT

    static final byte INS_SELECT

  APDU command INS : SELECT = 0xA4

  See Also:
    Constant Field Values

### INS_EXTERNAL_AUTHENTICATE

    static final byte INS_EXTERNAL_AUTHENTICATE

  APDU command INS : EXTERNAL AUTHENTICATE = 0x82

  See Also:
    Constant Field Values

Overview | Package | Class | Use | Tree | Deprecated | Index | Help

Java Card
v2.2.2
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

Copyright © 1993-2005 Sun Microsystems, Inc. 4150 Network Circle,
Santa Clara, CA, 95054, U.S.A. All Rights Reserved.